# Changing Fax Settings (Settings that Can Be Specified Using the [Menu] Button)

Configure the following settings to determine how to send faxes.
For the instructions on how to configure these settings, follow the steps in the procedures provided in "Configuring Send Settings" and "Configuring System Settings."

#### Basic Settings

"Register Unit Telephone Number"
"Register Unit Name"
"Select Line Type"
"Public Line Connection"
"Off-Hook Alarm"

#### TX Function Settings

"Change Defaults"
"ECM TX"
"Pause Time"
"Auto Redial"
"Sender ID"
"Check Dial Tone Before Sending"

#### System settings

"TX Start Speed"
"Restrict Fax TX/Telephone Dialing"
"Address Book PIN"
"Restrict New Destinations"
"Allow Fax Driver TX"
"Restrict Sending From History"
"Fax No. Confirmation Re-Entry"
"One-Touch/Coded Dial TX Confirmation"
"Restrict Sequential Broadcast"
0AE3-05L