# Printer Specification

Printer Specification
Printing Method | Indirect electrostatic system (On-demand fixing)
Paper Capacity | Paper cassette: Approx. 250 sheets (16 lb Bond to 21 lb Bond (60 g/m² to 80 g/m²))
Output Tray Capacity (a fresh stack of Letter size paper) | Approx. 100 sheets (20 lb Bond (75 g/m²))*1
Print Speed (Letter Plain Direct)*2 | 26 ppm
First Print Time (Letter) | 5.8 seconds or less*3
Output Resolution | 600 dpi x 600 dpi (1,200 dpi equivalent x 600 dpi)
Gradation | 256 gradations
Toner Cartridges | "Toner Cartridges"

*1 | The actual paper capacity varies depending on the installation environment and paper type used.
*2 | The print speed on Letter size plain paper on one-side printing is measured during continuous printing. Print speeds vary depending on the output resolution, the paper type and size, and the paper feeding direction. Print speeds on smaller paper sizes may be slower. Plus, the machine may experience downtime or decrease the print speed in the middle of a continuous print run to adjust the temperature inside the machine or maintain the optimal print quality.
*3 | May vary depending on the output environment.

0AE3-041