# Sending to Multiple Destinations at a Time (Sequential Broadcast)

See "Attention (Sequential Broadcast)" in advance.

You can send the same fax to multiple destinations simultaneously.
1
Place your fax.
"Placing Documents"
"Supported Document Types"
2
Press [] (FAX/COPY) to switch to the Fax mode screen.
3
Specify the destination.
"Specifying Destinations"
To specify a destination, following methods are available.
Entering the fax number
One-touch keys
Coded dialing codes
Group addresses
Address Book
4
Press [] or [] to highlight a method for specifying destinations, and then press [OK].

###### When specifying destinations from the Address Book or Coded Dial: "Specifying Destinations"
###### When specifying destinations with the numeric keys (Specify Next Destination (New)):
(1) Press [] or [] to highlight <Specify Next Destination (New)>, and then press [OK].
(2) Specify the next destination with the numeric keys, and then press [OK].
Repeat these steps to enter all the destinations.

5
Repeat step 4 to enter all the destinations.
6
Press [] (Start).
0AE3-05E