# Changing the Receive Mode

Select the receive mode that you want to use.

NOTE
###### The external telephone: The machine may not be able to send or receive faxes properly, depending on the type of telephone connected to it.

1
Press [] (FAX/COPY) to switch to the Fax mode screen.
2
Press [] or [] to highlight <RX Mode>, and then press [OK].
3
Press [] or [] to highlight the receive mode, and then press [OK].

###### If <Fax/Tel Auto Switch> is specified:

Proceed to specify the advanced settings. See "Advanced Settings for the Fax/Tel Auto Switch Mode."

###### If you select <DRPD: Select Fax>:

Press [] or [] to highlight a ring pattern, and then press [OK].
0AE3-06K