# Connecting the Power Cord

See "Attention (Connecting the Power Cord)" in advance.

After connecting the handset, connect the power cord.
1
Make sure that the machine is turned OFF.
2
Plug the female end of the power cord into the power socket on the back of the machine.
3
Plug the male end of the power cord into an AC power outlet.

Continued with the steps in the procedure below to turn ON the power and specify the initial settings. "Turning On the Machine and Specifying the Initial Settings"

0AE3-00U