# Auto Redial

Set auto redialing to automatically reattempt to connect to a destination if the line is busy or a send error occurs. You can also specify the how many time to redial a number and an interval between attempts.

###### How to access the option:

[] (Menu) -> <Fax TX Settings> -> <TX Function Settings> -> <Auto Redial>

###### Settings:

(Bold: Default setting)

Off | Disable Auto Redial. See "Redialing (Manual Redialing)" to redial the number manually.
On | Redial Times: 1 to 2 to 10 (times) | Set the number of redial attempts.
Redial Interval: 2 to 99 (min.) | Set the interval (in minutes) between redial attempts.
Redial When Err Occurs: Off, On | Specify whether to redial the number when a sending error occurs.

0AE3-063