# Push-button Telephone for Tone Dialing

See "Attention (Push-button Telephone for Tone Dialing)" in advance.

Some types of push-button telephones require a push-button line (for example, banks, airlines, or hotel reservations). When the machine is connected to a dial-up line, you can receive a fax using tone dialing. Follow the steps in the procedure below.
1
Press [] (FAX/COPY) to switch to the Fax mode screen.
2
Press [] (Hook) and check for the dial tone.
Check if you hear the dial tone.
3
Dial the information service from which you want to receive fax(es) using the numeric keys.
4
Respond to the prerecorded messages of the information service and press [] (Tone).
You can switch to tone dialing.
5
Enter the required numbers using the numeric keys.
6
Press [] (Start) to receive fax(es).
0AE3-059