# Fax RX Settings

NOTE
###### Menu options in the following chart: Default settings are highlighted in bold.

#### RX Function Settings

Settings | Descriptions
ECM RX | Set whether or not to use the electronic correction mode:
Off, On
"ECM RX"
Incoming Ring | Set whether or not to ring the external telephone or the handset when <RX Mode> is set to <Auto> or <Fax/Tel Auto Switch>:
Off On: Ring Times: 1 to 2 to 99 (times)
"Incoming Ring"
Remote RX | Set whether or not to use the "remote receiving function" enabling you to receive fax documents by dialing an ID number even in the middle of a telephone call:
Off On: Remote RX ID: 00 to 25 to 99
"Remote RX"
Switch to Auto RX | Set the incoming call ring time before the machine switches to the fax mode automatically. This option can be enabled when the <RX Mode> is set to <Manual>:
Off On: Ring Time till Auto RX: 1 to 15 to 99 (sec.)
"Switch to Auto RX"

#### RX Print Settings

Settings | Descriptions
2-Sided Printing | Set whether or not to print documents on both sides of the paper. This enables you to save paper.
Off, On
"2-Sided Printing"
Reduce RX Size | Set an automatic reduction rate for printing received faxes:
Off On: Reduction Ratio: Auto, 97, 95, 90, 75 (%) Reduction Direction: Vertical/Horizontal, Vertical Only
"Reduce RX Size"
RX Page Footer | Set whether or not to include a footer on received faxes:
Off, On
"RX Page Footer"
Continue Print. When Toner Is Nearly Out | Set whether or not to continue printing when toner is low:
Off, On
"Continue Print. When Toner Is Nearly Out"

0AE3-0A2