# Configuring Send Settings

This section describes how to configure the send settings.
See the following for more information:
"The Steps to Take for Configuring the Send Settings"
"Options"

## The Steps to Take for Configuring the Send Settings

Follow the steps in the procedure below to configure the send settings.
The procedure describes the steps to change the "ECM TX" setting.
1
Press [] (Menu).
2
Press [] or [] to highlight <Fax TX Settings>, and then press [OK].
3
Press [] or [] to highlight <TX Function Settings>, and then press [OK].
4
Press [] or [] to highlight <ECM TX>, and then press [OK].
5
Press [] or [] to highlight <Off> or <On>, and then press [OK].

| Select <Apply> when <Apply> appears on the screen after you have specified the setting and press [OK].

6
Press [] (Menu) to close the Menu screen.
The procedure is complete.

## Options

Configure the following options to send a fax:

Fax Settings
Basic Settings | "Register Unit Telephone Number"
"Register Unit Name"
"Select Line Type"
"Public Line Connection"
"Off-Hook Alarm"
TX Function Settings | "Change Defaults"
"ECM TX"
"Pause Time"
"Auto Redial"
"Sender ID"
"Check Dial Tone Before Sending"

0AE3-05R