# Cleaning the Platen Glass

See "Attention (Cleaning the Machine)" in advance.

Follow this procedure to clean the platen glass and the under surface of the feeder.
1
Turn OFF the power switch and disconnect the power cord.
2
Open the feeder.
3
Clean the platen glass and the under surface of the feeder.

(1) | Clean the areas with a cloth dampened with water.
(2) | Wipe the areas with a soft, dry cloth.

IMPORTANT
###### Precautions when cleaning the platen glass: Be careful not to fold the transparent sheet (A) at the left side of the platen glass.

4
Close the feeder.
5
Connect the power cord and turn ON the power switch.
0AE3-0H0