# Cleaning the Interior

Before cleaning the interior of the machine, see "Attention (Cleaning the Machine)."

Clean the machine's print area periodically to prevent toner powder and paper dust from accumulating inside.
1
Turn OFF the power switch, and then disconnect the power cord.
2
Hold the operation panel.
3
Lift the scanning platform.

If you cannot lift the scanning platform: Ensure that the feeder is completely closed. Do not try to forcefully lift the scanning platform, as this may damage the machine.
| If you set thick documents such as a book, the feeder may not be completely closed. Remove the documents.

4
Hold the grip on the left front side of the toner cover.
5
Open the toner cover.
6
Remove the toner cartridge.
7
Remove any toner or paper debris from interior of the machine, with a clean, soft, dry, and lint-free cloth.
8
Insert the toner cartridge.
Fit the protrusions (A) on each side of the toner cartridge into the guides located on each side of the machine. Slide the toner cartridge into the machine, until the toner cartridge meets the back of the machine.
9
Close the toner cover.

If you cannot close the toner cover:
Make sure that the toner cartridge is properly installed in the machine. Do not try to forcefully close the toner cover, as this may damage the machine.

10
Lower the scanning platform.
11
Connect the power cord, and then turn ON the power switch.
0AE3-0CY