# Sending a Fax at a Preset Time

You can automatically send a pre-scanned document at a preset time.
1
Place your fax.
"Placing Documents"
"Supported Paper Types"
2
Press [] (FAX/COPY) to switch to the Fax mode screen.
3
Specify the scanning settings as needed.
"Changing the Scan Settings (Fax)"
4
Press [] or [] to highlight <Delayed TX>, and then press [OK].
5
Press [] or [] to highlight <On>, and then press [OK].
6
Enter the time at which you want to send the document, and then press [OK].
"Entering Text"
7
Specify the destination.
"Specifying Destinations"
Specify destinations in the following ways:
by entering the fax number
by selecting a one-touch key
by selecting a coded dial code
by selecting a group address
from the Address book
under sequential broadcasting
8
Press [] (Start).

###### When your fax is placed in the feeder:

The scan starts. Your fax is sent to the destination when the scan is complete.

###### When your fax is placed on the platen glass:

Perform the following procedure.

(1) | Press [] or [] to highlight the size of the original document, and then press [OK].
(2) | Place the next page on the platen glass, and then press [] (Start). Press [] (Start) for each page.
(3) | When all documents are scanned completely, press [] or [] to highlight <Start Sending>, and then press [OK]. Your fax is sent to the destination.

NOTE
###### If the machine memory becomes full while scanning a document: <Memory is full.> appears in the display and you cannot send the document at a delayed time. "Onscreen Messages"
###### The number of operation that you can register: You can only register one preset sending operation at a time.
###### Job operation while the delayed sending is set: To print, copy, or send other documents after setting the machine for delayed sending, simply follow the procedures described in this manual.
###### To cancel a delayed sending: See "Checking and Canceling Fax Jobs."
###### If the machine is turned off at the preset time: If the fax is stored in the memory, the fax will be sent when you turn on the machine.

0AE3-056