# Paper Curls

Try one of the following to solve the problem.

#### <Cause 1> Damp paper is used.

Solution 1 | Replace the paper with new paper in an unopened package. "Supported Paper Types"
Solution 2 | Follow the procedures below when plain paper (16 lb Bond to 24 lb Bond (60 g/m² to 90 g/m²)) is loaded.
1. | Display the [Page Setup] tab.
2. | Set [Paper Type] to [Plain Paper L].
Solution 3 | Change the <Special Mode V> setting from the operation panel. "Settings That Can Be Specified From the Operation Panel"

#### <Cause 2> The paper type loaded is not appropriate.

Solution | Make sure that the number and type of the paper loaded in the paper cassette meets the paper requirements. "Supported Paper Types"

0AE3-0C6