# Remote RX

Specify whether to receive faxes remotely by dialing the ID number using the push-buttons of the external telephone connected to the machine when an incoming call comes. If you use the pulse line, press "" (Tone) and then dial the Remote RX ID.

###### How to access the option:

[] (Menu) -> <Fax RX Settings> -> <RX Function Settings> -> <Remote RX>

###### Settings:

(Bold: Default setting)

Off | Disable remote retrieval.
On | Remote RX ID: 00 to 25 to 99 | Enable remote retrieval. You can specify the ID number in <Remote RX ID>.

0AE3-074