# Paper Creases

Try one of the following to solve the problem.

#### <Cause 1> The paper is not loaded properly.

Solution | Load the paper properly. "Loading Paper In the Paper Cassette"

#### <Cause 2> Damp paper is used.

Solution | Replace the paper with new paper in an unopened package. "Supported Paper Types"

#### <Cause 3> The paper type loaded is not appropriate.

Solution | Make sure that the number and type of the paper loaded in the paper cassette meets the paper requirements. "Supported Paper Types"

#### <Cause 4> There is a foreign object inside the machine.

Solution | Remove the foreign object from the machine.

#### <Cause 5> Depending on the paper type or the operating environment, the paper may be creased.

Solution | Change the <Special Mode V> setting from the operation panel. "Settings That Can Be Specified From the Operation Panel"

0AE3-0C7