# Setting up the Machine

Follow the steps in the procedure below to take the machine out of the shipping box, install it, and connect the power cord.

###### Step 1 | Make sure that all the supplied accessories are included inside the box. | "Checking the Supplied Accessories"
###### Step 2 | Carry the machine to the installation location and remove the packing materials. | "Carrying the Machine to the Installation Location and Removing the Packing Materials"
###### Step 3 | Prepare to use the toner cartridge. | "Preparing to Use the Toner Cartridge"
###### Step 4 | Load paper. | "Loading Paper"
###### Step 5 | Connect the handset. | "Connecting the Handset"
###### Step 6 | Connect the power cord. | "Connecting the Power Cord"

0AE3-00E