# Connecting the Handset

After loading paper, connect the handset to the machine. The handset can be installed on the left side of the machine.
1
Remove the covers (2 locations).

If you cannot remove the covers:
Use a flat-head screwdriver to remove the covers. Be careful when you use flat-head screwdriver to remove the covers as this may damage the machine.

2
Insert the pins in the holes in the cradle. Push the pins in only up to the first stop (A).
3
Align the pins with the holes in the machine and connect the cradle to the machine. Push the pins in only up to the first stop.
4
Push the pins to the end.
5
Place the handset on the cradle.
6
Connect the handset’s telephone line to the handset jack.
7
Attach the clamp to the machine.
8
Attach the handset’s telephone line and close the clamp.

Continued with the steps in the procedure below to connect the power cord. "Connecting the Power Cord"

0AE3-00S