# Fax TX Settings

NOTE
###### Menu options in the following chart: Default settings are highlighted in bold.

#### Basic Settings

Settings | Descriptions
Register Unit Telephone Number | Set a fax number for the machine: "Registering the Sender Information" "Register Unit Telephone Number"
Register Unit Name | Set your name or your company's name as the machine name (sender's name): "Registering the Sender Information" "Register Unit Name"
Select Line Type | Select a line type:
Pulse, Tone
"Select Line Type"
Public Line Connection | If the external telephone does not ring or you cannot make a call using the external telephone when the fax receive mode is set to <Fax/Tel Auto Switch>, set <Public Line Connection> settings to <Adapter 1> or <Adapter 2>:
Direct, Adapter 1, Adapter 2
"Public Line Connection"
Off-Hook Alarm | Set whether or not to sound an alarm when the telephone handset is off the hook and adjust the volume:
Off On: Off-Hook Alarm Volume: 1 to 5
"Off-Hook Alarm"

#### TX Function Settings

Settings | Descriptions
Change Defaults | Store new transmission settings: "Change Defaults"
ECM TX | Set whether or not to use the electronic correction mode:
Off, On
"ECM TX"
Pause Time | Set a duration for pauses added to fax numbers:
1 to 2 to 15 (sec.)
"Pause Time"
Auto Redial | Set whether or not to automatically redial unconnected fax numbers:
Off, On
"Auto Redial"
Redial Times | Set the number of times to redial:
1 to 2 to 10 (times)
"Auto Redial"
Redial Interval | Set the interval between redials:
2 to 99 (min.)
"Auto Redial"
Redial When Err Occurs | Set whether or not to redial when a send error occurs:
Off, On
"Auto Redial"
Sender ID | Set whether or not to add sender information to faxes. This helps the recipient to identify the sender:
Off, On
"Sender ID"
Print Location | Select the location where the Sender ID is printed:
On Image, Above Image
"Sender ID"
Mark No. as | Select the text to add in front of the number:
FAX, TEL
"Sender ID"
Check Dial Tone Before Sending | Set whether or not verify a dial tone before dialing fax numbers:
Off, On
"Check Dial Tone Before Sending"

#### Fax Setup Guide

Specify initial fax settings and connect the telephone cable.
"Turning On the Machine and Specifying the Initial Settings"
0AE3-0A1