# Switch to Auto RX

Specify how long an incoming call should ring before the machine automatically switches to fax mode. This option can be enabled when the <RX Mode> is set to <Manual>.

###### How to access the option:

[] (Menu) -> <Fax RX Settings> -> <RX Function Settings> -> <Switch to Auto RX>

###### Settings:

(Bold: Default setting)

Off | Remote receiving is disabled.
On | Ring Time till Auto RX: 1 to 15 to 99 (sec.) | Remote receiving is enabled. You can specify the time before the machine starts receiving a fax in <Ring Time till Auto RX>.

0AE3-075