# Restricting Sequential Broadcasts

Specify whether or not to restrict to send a fax to multiple destinations simultaneously.
1
Press [] (Menu).
2
Press [] or [] to highlight <System Settings>, and then press [OK].

###### If a System Manager PIN is specified:

Use the numeric keys to enter the System Manager PIN, and then press [OK].
3
Press [] or [] to highlight <Restrict TX Function>, and then press [OK].
4
Press [] or [] to highlight <Restrict Sequential Broadcast>, and then press [OK].
5
Press [] or [] to highlight whether to restrict sequential broadcasts or not, and then press [OK].

<Off> | Allow users to send faxes to multiple destinations.
<Confirm Sequential Broadcast> | Allow users to send faxes to multiple recipients and requires a confirmation.
<Reject Sequential Broadcast> | Prevent users from sending faxes to multiple recipients.

6
Press [] (Menu) to close the Menu screen.
0AE3-09H