# Forwarding Received Faxes Stored in Memory to Other Destinations (Manual Forwarding)

When a fax is stored in memory, you can manually forward it to a specified destination.

NOTE
###### Destinations that can be specified: You can forward a fax to only one destination to the address book, one-touch key, or coded dialing code.
###### To restore received fax data in memory: See "Memory Lock Settings."

1
Press [] (Status Monitor/Cancel).
2
Press [] or [] to highlight <Fax Job Status/History>, and then press [OK].
3
Press [] or [] to highlight <RX Job Status>, and then press [OK].
4
Press [] or [] to highlight the job you want to forward, and then press [OK].
You cannot forward received faxes when
the machine is in the middle of receiving another fax
the machine starts printing a job after it has received a fax
5
Press [] or [] to highlight <Forward>, and then press [OK].
6
Specify the destination from the address book, and then press [OK].
"Specifying Destinations Using the Address Book"
0AE3-06R