# Configuring System Settings

This section describes how to configure the system settings.
See the following for more information.
"The Steps to Take for Configuring the System Settings"
"Options"

## The Steps to Take for Configuring the System Settings

Follow the steps in the procedure below to configure the system settings.
The procedure describes the steps to change the "TX Start Speed" setting.
1
Press [] (Menu).
2
Press [] or [] to highlight <System Settings>, and then press [OK].

###### If a System Manager PIN is specified:

Use the numeric keys to enter the System Manager PIN, and then press [OK].
3
Press [] or [] to highlight <Communication Management Settings>, and then press [OK].
4
Press [] or [] to highlight <Fax Settings>, and then press [OK].
5
Press [] or [] to highlight <TX Start Speed>, and then press [OK].
6
Press [] or [] to highlight the send start speed, and then press [OK].

| Highlight <Apply> when <Apply> appears on the screen after you have specified the setting and press [OK].

7
Press [] (Menu) to close the Menu screen.
The procedure is complete.

## Options

Configure the following options to send a fax:

System Settings
Communication Management Settings | Fax Settings | "TX Start Speed"
Restrict TX Function | "Restrict Fax TX/Telephone Dialing" |
"Address Book PIN"
"Restrict New Destinations"
"Allow Fax Driver TX"
"Restrict Sending From History"
"Fax No. Confirmation Re-Entry"
"One-Touch/Coded Dial TX Confirmation"
| "Restrict Sequential Broadcast" |

0AE3-066