# Advanced Settings for the Fax/Tel Auto Switch Mode

Set the advanced settings for the Fax/Tel Auto Switch mode.
1
Press [] (FAX/COPY) to switch to the Fax mode screen.
2
Press [] or [] to highlight <RX Mode>, and then press [OK].
3
Press [] or [] to highlight <Fax/Tel Auto Switch>, and then press [OK].
4
Press [] or [] to highlight the option, and then press [OK].

<Ring Start Time> | Specify how long the machine will attempt to detect a fax tone before the handset starts ringing. Set the duration somewhere between 4 to 30 seconds and press [OK].
<Incoming Ring Time> | Set how long the handset will ring during an incoming call. Set the duration somewhere between 15 to 300 seconds and press [OK].
<Action After Ring> | Specify how the machine behaves when an incoming call is not answered. Select <End> or <RX> and press [OK]. <End>: Disconnect the call. <RX>: Receive an incoming fax.

5
Press [] or [] to highlight <Apply>, and then press [OK].
The changes are saved.
0AE3-06L