# Operation Panel

(1) | [FAX/COPY] key | Press to switch the mode to copy or fax.
(2) | LCD | During normal operation, displays messages and prompts. When adjusting the settings, displays your selections, text, and numbers.
(3) | [Reset] key | Resets the settings.
[Back] key | Press to return to the previous screen.
[] key | Press to scroll up or to increase the value.
[] key | Press to scroll down or to decrease the value.
[] key | Press to return to the previous screen, or move the cursor to the left. Press to decrease the volume while the fax ring tone sounds.
[] key | Press to proceed to the next screen, or move the cursor to the right. Press to increase the volume while the fax ring tone sounds.
[OK] key | Press to confirm an action or setting.
[Status Monitor/Cancel] key | Press to view the status of jobs or cancel jobs. You can also check the status of the machine.
[Paper Settings] key | Press to specify paper size and type for the paper cassette.
(4) | [Processing/Data] indicator | Blinks during transmission and turns on when the machine has waiting jobs.
[Error] indicator | Blinks when an error occurs.
(5) | [Menu] key | Press to specify or register various settings.
[Report] key | Press to manually print reports and lists. You can also specify whether to report automatically.
[Image Quality] key | Press to select the image quality for copy or the scanning resolution for the sending document.
[2-Sided] key | Press to print on both sides of paper.
Numeric keys ([0]-[9]) | Press to enter characters and numbers.
[*] key | Press to switch the character entry mode, and switch between pulse and tone dialing to send a fax.
[#] key | Press to enter symbols.
[Quiet Mode] key | Press to reduce the noise when performing job. This does not affect the speaker or the key volume.
[Clear] key | Press to delete entered characters and numbers.
[Energy Saver] key | Press to manually set or cancel the Sleep mode. The Energy Saver indicator lights green while in the sleep mode.
[Stop] key | Press to cancel jobs.
[Start] key | Press to start copying or send a fax.

## Fax Operation Panel

(1) | [One-touch Speed Dial] keys | Press to select destinations registered in one-touch keys.
(2) | [Address Book] key | Press to search for recipients who are registered under one-touch keys or coded dial codes.
(3) | [Coded Dial] key | Press to specify and enter a recipient's code for coded speed dialing.
(4) | [Redial/Pause] key | When faxing, press to redial the last three numbers called or insert a pause in a fax number.
(5) | [Hook] key | Press when you want to dial without lifting up the handset of the external telephone or the handset.

0AE3-01J