# Attention (Preparing to Use the Toner Cartridge)

See "Maintenance and Inspections" in "Important Safety Instructions."

WARNING
###### When cleaning up spilled or scattered toner: If you accidentally spill or scatter toner, carefully gather the toner particles together or wipe them up with a soft, damp cloth in a way that prevents inhalation. Never use a vacuum cleaner that does not have safeguards against dust explosions to clean up spilled toner. Doing so may cause a malfunction in the vacuum cleaner, or result in a dust explosion due to static discharge.

CAUTION
###### Precautions to take when you get toner onto your hands or into clothing: If toner comes in contact with your hands or clothing, wash them immediately in cold water. Do not use warm water, as it will set the toner and make it difficult to remove the toner stains.
###### Do not allow the toner to scatter. Do not pull out the sealing tape forcefully or stop pulling the tape halfway, as this may cause toner to spill out. If toner gets into your eyes or mouth, flush them immediately with cold water and consult a physician.
###### Use caution when lowering the scanning platform: Keep your fingers clear of the scanning platform to avoid injury.

IMPORTANT
###### Use caution when pulling out the sealing tape. Do not pull the sealing tape at an angle or up and down. If the tape breaks, it may not be pulled out completely. If the sealing tape is still hanging outside the toner cartridge, pull it out completely. Do not leave any sealing tape in the cartridge, as this may affect print quality. If you are using the Fax, please note that you can only print the received data once, because the received data is deleted once it is printed.
###### Disposing of the removed sealing tape: Dispose of the sealing tape according to all applicable regulations.
###### Do not leave the toner cover open for an extended period of time when the toner cartridge is installed. Exposing the toner cartridge for extended periods may affect print quality.

0AE3-00L