# Attention (Loading Paper)

CAUTION
###### Be careful when handling paper. Handle paper carefully to avoid cutting your hands with the edges of the paper.
###### Precautions when closing the dust cover: Keep your fingers clear of the dust cover to avoid injury.

IMPORTANT
###### Adjust the paper guides tightly to the width of the paper. If the paper guides are too loose or too tight, the document may be misfed or become jammed. Printouts may be askew depending on the printing environment. Properly load paper to reduce the symptom.
###### When using paper that has been poorly cut: If you use paper that has been poorly cut, multiple sheets of paper may be fed at once. In this case, fan the paper thoroughly, and then align the edges of the stack properly on a hard, flat surface.
###### Do not exceed the loading limit marks when loading paper. Make sure that the paper stack does not exceed the loading limit marks. If the paper stack exceeds the loading limit marks, this may result in misfeeds.
###### When printing on envelopes: Load envelopes with the front side (non-glued side) facing up. You cannot print on the reverse side of envelopes. Also, be sure to close the flap before loading envelopes.

NOTE
###### For more information on supported paper types: "Supported Paper Types"
###### Abbreviations on the paper guides inside the paper cassette:
Paper Size | Paper Guide
Legal | LGL
Letter | LTR
Executive | EXEC
Statement | STMT

0AE3-02C