# Communication Management Report

Specify whether to print the Communication Management report automatically.
You can also print the report manually.
"Printing a Communication Management Report"
The report includes the following:
Start time
Name
No.
Mode
Page
Result
OK
Transmission finished successfully.
NG
Transmission failed.
If an error code is displayed, see the following.
"Error Codes"
1
Press [] (Report).
2
Press [] or [] to highlight <Report Settings>, and then press [OK].
3
Press [] or [] to highlight <Communication Management Report>, and then press [OK].
4
Specify how you want to print the report.

###### If you do not want to print the report automatically:

(1) | Press [] or [] to highlight <Auto Print (40 Transmissions)>, and then press [OK].
(2) | Press [] or [] to highlight <Off>, and then press [OK].
(3) | Proceed to step 5.

###### If you want to print the report automatically:

(1) | Press [] or [] to highlight <Auto Print (40 Transmissions)>, and then press [OK].
(2) | Press [] or [] to highlight <On>, and then press [OK].
(3) | Proceed to step 5.

###### If you want to print the sending and receiving reports separately:

(1) | Press [] or [] to highlight <Separate TX/RX>, and then press [OK].
(2) | Press [] or [] to highlight <Off> or <On>, and then press [OK]. <Off>: Prints the sending and receiving reports together. <On>: Prints the sending and receiving reports separately.
(3) | Proceed to step 5.

5
Press [] (Report) to close <Report Settings> screen.
0AE3-03E