# Configuring Receiving Settings

This section describes how to configure the receiving settings.
See the following for more information:
"Setting Procedure for Receiving Faxes"
"Options"

## Setting Procedure for Receiving Faxes

Follow the steps in the procedure below to configure the fax receiving settings.
The procedure describes the steps to change the "ECM RX" setting.
1
Press [] (Menu).
2
Press [] or [] to highlight <Fax RX Settings>, and then press [OK].
3
Press [] or [] to highlight <RX Function Settings>, and then press [OK].
4
Press [] or [] to highlight <ECM RX>, and then press [OK].
5
Press [] or [] to highlight <Off> or <On>, and then press [OK].

| Select <Apply> when <Apply> appears on the screen after you have specified the setting and press [OK].

6
Press [] (Menu) to close the Menu screen.

## Options

Configure the following options to receive a fax:

Fax Settings
RX Function Settings | "ECM RX"
"Incoming Ring"
"Remote RX"
"Switch to Auto RX"
RX Print Settings | "2-Sided Printing"
"Reduce RX Size"
"RX Page Footer"
"Continue Print. When Toner Is Nearly Out"

0AE3-071