# Incoming Ring

Specify whether or not the external telephone or the handset rings on an incoming call when <RX Mode> is set to <Auto> or <Fax/Tel Auto Switch>.
You can set the incoming call ring time.
The machine automatically starts receiving a fax after the external telephone keeps ringing for a specified length of time.

###### How to access the option:

[] (Menu) -> <Fax RX Settings> -> <RX Function Settings> -> <Incoming Ring>

###### Settings:

(Bold: Default setting)

Off | The telephone does not ring on an incoming call.
On | Ring Times: 1 to 2 to 99 (times) | The telephone rings on an incoming call. You can set the incoming call ring time in rings in <Ring Times>.

0AE3-073