# Relocating the Machine

See "Attention (Relocating the Machine)" in advance.

When changing the location of the machine or moving the machine for maintenance, be sure to perform the following procedure.
1
Turn OFF the machine and any connected computer.
2
Disconnect all cables and the power cord from the machine.

###### How to remove the cables and cord:

USB cable* |
(1) | Remove it from the machine.
Handset cable and Telephone cables* |
(2) | Remove it from the machine.
Power cord |
(3) | Unplug the power plug from the AC power outlet.
(4) | Remove it from the machine.

* Whether the cable is connected or not varies depending on your environment.
3
Fold the paper stopper.

NOTE
###### If paper is in the output tray: Remove the paper from the output tray.

4
Open the front cover and the lower front cover.
5
Remove any paper from the paper cassette.

NOTE
###### If the paper guide at the front projects from the paper cassette: Push the paper guide into the paper cassette.

6
Close the front cover and the lower front cover.
7
Move the machine.
Make sure that all covers and trays are closed or removed, and hold the lift handles with the front side of the machine facing you.
Check the weight of the machine to carry it safely.
"Machine Specifications"

8
Carefully set the machine down on the new installation site.

NOTE
###### When reinstalling the machine: See the supplied Starter Guide.

## When Transporting the Machine to a Long Distance

To prevent damage to the machine during transportation, refer to the following:
Remove the toner cartridge.

| See also "Storing Toner Cartridges."

Securely pack the printer in its original box with the original packing materials.

| If the original box and packing materials are not available, find an appropriate box along with packing materials and pack the machine and the parts appropriately.

0AE3-0E8