# Fax Specifications

Fax Specifications
Line Used | Public Switched Telephone Network (PSTN)*1
Communication Mode | Super G3, G3
Compression Method | MH, MR, MMR
Modem Speed | Super G3: 33.6 Kbps, G3: 14.4 Kbps Automatic Fallback
Transmission Speed | Approx. 3 seconds per page*2 (ECM-MMR, transmitting from the memory at 33.6 Kbps)
Sending from Memory/Receiving in Memory | Maximum approx. 512 pages*2 (Total pages of transmission/reception) (Maximum number of fax jobs that can be sent from the memory: 10 jobs/ Maximum number of fax jobs that can be received into the memory: 90 jobs)
Fax Resolution | (Normal): 200 dpi x 100 dpi (Fine): 200 dpi x 200 dpi (Photo): 200 dpi x 200 dpi (Superfine): 200 dpi x 400 dpi
Dialing | One-touch keys (40 destinations) Coded dialing (200 destinations) Group dialing (239 groups, 50 destinations in each group) Address book dialing Regular dialing (with numeric keys) Automatic redialing Manual redialing Sequential broadcast (250 destinations)
Receiving | Automatic reception Remote reception by telephone (Default ID: 25)
Reports | TX Result Report Communication Management Report (Auto output every 40 destinations) RX Result Report

*1 | The Public Switched Telephone Network (PSTN) currently supports 28.8 Kbps modem speed or lower. Note that speeds can vary depending on the telephone line conditions.
*2 | Based on ITU-T (ITU Telecommunication Standardization Sector) Standard Chart No. 1, MMR standard mode.

0AE3-042