# Introduction of the Optional Accessories

The following optional accessories are available to make full use of the printer functions.

| For the optional accessories, contact your local authorized Canon dealer.

## Paper Feeder

You can load up to 250 sheets of plain paper (90 g/m²) of the following sizes in the paper feeder.

Standard sizes | A4, B5, A5, Legal, Letter, Executive, Statement, Foolscap, Envelope DL, Envelope COM-10, Envelope ISO-C5, and Envelope ISO-B5
Custom paper sizes | Width 100.0 to 215.9 mm, Length 148.0 to 355.6 mm*

* | If you are using the UFR II printer driver, you can load custom size paper that is 148.0 to 215.9 mm wide and 148.0 to 215.9 mm long also in landscape orientation.

Paper Feeder Unit PF-701

IMPORTANT
###### Use a paper feeder designed for this printer. Be sure to use a paper feeder designed for this printer.

NOTE
###### How to install the paper feeder "Installing the Paper Feeder"

## PS ROM (LBP7660Cdn Only)

By installing PS ROM, "PostScript 3 Emulation" which makes it possible to print with PostScript is available.

PS Printer Kit-AQ1

NOTE
###### How to install PS ROM "Installing ROM"

## Barcode ROM

The following function is available by installing Barcode Printing Kit-F1.
<Bar code fonts for bar code printing>
OCR-B
Symb. FontInform
Symbole stethos
BarDIMM ©1997
USPS ZEBRA+4Stat

Barcode Printing Kit-F1

NOTE
###### How to install Barcode Printing Kit-F1 "Installing ROM"

## SD Card (LBP7680Cx Only)

You can use an SD card that can be built in the printer to save the received print jobs temporarily. By installing the SD card, you can use various functions such as print job spooling, encrypted secured print, secured print, and electronic sort.

| Before you dispose of this product, prevent personal information from being leaked by physically destroying the product.

SD CARD-B1

NOTE
###### How to install the SD card "Installing SD Card"

0258-012