# Attention (Drawer)

See "Important Safety Instructions" also.

IMPORTANT
###### When loading paper for the first time after installing the paper feeder Before loading paper, be sure to turn ON the printer once. ###### Do not touch the black rubber pad (A) in the paper drawer. This may result in misfeeds. ###### Do not pull out the drawer during printing. This may result in paper jams or damage to the printer. ###### When using paper that is poorly cut Multiple sheets of paper may be fed at a time. In this case, fan the paper thoroughly, and then align the edges of the stack properly on a hard, flat surface.

0258-035