# Paper Curls

Perform one of the following solutions according to the cause.

#### <Cause 1> Damp paper is used.

Solution | Replace the paper with new paper in an unopened package. "Precautions for Paper"

#### <Cause 2> Appropriate paper is not being used.

Solution | Replace the paper with that which can be used with this printer. "Usable Paper"

#### <Cause 3> Depending on the paper type or the operating environment, the paper may curl as either of the following.

Solution 1 | Perform the following procedure in the printer driver.
1. | Display the [Paper Source] sheet.
2. | Set [Paper Type] to one of the following settings.
Currently Selected Setting | Setting to be Selected
[Plain L] | [Plain L2]
[Plain] | [Plain L]
[Plain H] | [Plain]
[Heavy 1] | [Plain H]
[Heavy 2] | [Heavy 1]
[Heavy 3] | [Heavy 2]
[Envelope H] | [Envelope]
[Coated 2] | [Coated 1]
[Coated 3] | [Coated 2]
[Coated 4] | [Coated 3]
| If you change the settings, the toner may not fix onto paper well, and the printing may come out faint.
Solution 2 | Select [Curl Correction] under [Special Print Mode] set it to [On] and print again. "[Setup] Menu ([User Maintenance] Options)"
| If you change the settings, the toner may not fix onto paper well, and the printing may come out faint.
| If you specify this setting, printing speed drops.

#### <Cause 4> Depending on the paper type or the operating environment, the paper may curl as either of the following.

Solution | Perform the following procedure in the printer driver.
1. | Display the [Paper Source] sheet.
2. | Set [Paper Type] to one of the following settings.
Currently Selected Setting | Setting to be Selected
[Plain L2] | [Plain L]
[Plain L] | [Plain]
[Plain] | [Plain H]
[Plain H] | [Heavy 1]
[Heavy 1] | [Heavy 2]
[Heavy 2] | [Heavy 3]
[Envelope] | [Envelope H]
[Coated 1] | [Coated 2]
[Coated 2] | [Coated 3]
[Coated 3] | [Coated 4]
| When the settings are changed, sometimes residual images appear on non-printed areas.

0258-0CF