# Performing the Configuration Using the Printer's Control Panel (the Settings to Be Performed First)

When configuring the spooler function using the printer's control panel, use the following menu hierarchy.
Pressing [ ] (: Settings) displays the common Setup menu.
indicates that the procedure is performed by pressing [ ] or [ ] on the control panel.
indicates that the procedure is performed by pressing [OK] on the control panel.

IMPORTANT
###### After performing the configuration To enable the settings, perform a hard reset or restart the printer. For details on a hard reset, see "Canceling All the Jobs (Hard Reset)." ###### To go back up the hierarchy Press [ ] (: Back). ###### About the control panel For details on the control panel, see "Control Panel."

1
Press [ ] (: Settings), select [Network] using [ ] and [ ], and then press [OK].
When the message is displayed, press [OK].

| You can specify the settings when the printer is either online (the Online indicator is on) or offline (the Online indicator is off).

2
Select [Spooler] using [ ] and [ ], and then press [OK].
3
Specify the setting for the spooler function using [ ] and [ ], and then press [OK].
4
Perform a hard reset or restart the printer.
After performing a hard reset or restarting the printer, the settings are effective.

NOTE
###### For details on a hard reset See "Canceling All the Jobs (Hard Reset)."

0258-0KC