# Adjusting the Color or Color Mismatch (Calibration)

There are the following four methods for performing calibration.

Calibration Types | Overview | Calibration time (rough estimate)
Color Mismatch Correction | A color mismatch is adjusted by controlling the shifts of the print start positions of each color. Execute when color mismatch occurs. | Approximately 54 seconds
Density Control | Controls the maximum print density and median print density. Execute when the colors have changed and the data is not printed in the correct colors (specified colors). | Approximately 56 seconds
Density Median Control | Controls the median print density. Execute when the colors of the median print density have changed and the data is not printed in the correct colors (specified colors). | Approximately 56 seconds
Full Calibration | Performs [Color Mismatch Corr.] and [Density Control]. Execute when you want to adjust color mismatch and control the print density (adjust color hues) at once. | Approximately 100 seconds

This section describes the procedure for performing calibration manually.
You can perform calibration from the control panel and the Remote UI.
Performing Calibration Using the Control Panel
Performing Calibration Using the Remote UI

IMPORTANT
###### Precautions when performing calibration If you perform calibration frequently, this may affect the life of the toner cartridges. Perform calibration after making sure that the toner remains in the toner cartridges.
|  | You can check the status of each color toner cartridge from [Remaining Toner] on the Remote UI portal page. "Remote UI Portal Page"
|  | If you perform calibration in the state where the toner cartridges have reached the end of their life, calibration may not finish properly. In this case, replace the toner cartridges, and then perform calibration again. "Replacing Toner Cartridges"

NOTE
###### Perform calibration at the designated time or immediately after the printer is turned ON. You can set the printer to automatically perform calibration at the designated time everyday or to perform calibration immediately after the printer is turned ON. "Specifying Times and Performing Automatic Calibration" "Automatically Performing Calibration Immediately after the Printer Is Turned ON"

## Performing Calibration Using the Control Panel

1
Press [ ] (: Utility).
2
Select [Calibration] using [ ] and [ ], and then press [OK].
3
Select an item which you want to adjust from [Color Mismatch Corr.], [Density Control], [Density Median Cont.], and [Full Calibration] using [ ] and [ ], and then press [OK].
4
Select [Yes] using [ ], and then press [OK].

→ | Calibration is performed.

## Performing Calibration Using the Remote UI

1
Start the Remote UI and log on in system manager mode.
"Starting the Remote UI"
2
Select [Calibration] from [Output/Control] under the [Settings/Registration] menu.
3
Perform calibration.

(1) | Select the calibration which you want to perform.
(2) | Click [Execute].

→ | Calibration is performed.

0258-0LJ