# Printing the PS/EPS File Using the Direct Print Function

IMPORTANT
###### When Using LBP7660Cdn In order to print PS/EPS files directly, it is necessary to install the optional PS ROM.

1
Start the Remote UI.
"Starting the Remote UI"
2
Select [PS File] from the [Direct Print] menu.
3
Specify [Select PS/EPS File].
Click [Browse...], select the file, and click [Open...].
4
Specify the setting for [Color Settings].

[Color Mode] | Specify color printing or B&W printing.
[Auto (Color/Black and White)]: | It automatically switches between color and black and white printing depending on the type of document.
[Black and White]: | Even color documents are printed in black (Bk) only.

5
Specify the settings for [Print Settings] as the following, as needed.

[Copies] | Specify the number of copies to be printed.
[Print 2-Sided] | Specify 1-sided or 2-sided printing.
[Binding Location] | Select the binding location from [Short Edge] and [Long Edge].
[Store in Box] | When storing it in a box, check the [Store in Box] check box before selecting the box where you want to store it.

6
Click [Start Printing].

| Do not keep clicking [Start Printing] while the file is transferring. Sometimes it takes time to transfer a file, but if you keep clicking during the transfer, a file failure may occur and it may be impossible to transfer it.

→ | When the print job has finished sending, the display switches and the following message is displayed.
| Press [To Job List] to check the print job that was sent.

0258-0F5