# Checking the MAC Address

You need the MAC address of the printer to set the IP address using NetSpot Device Installer or the ARP/PING command. There are the following two methods for checking MAC addresses.
"Checking the Network Ethernet Driver Screen from a Remote UI"
"Printing a Network Status Print from the Printer's Control Panel and Checking It"

## Checking the Network Ethernet Driver Screen from a Remote UI

1
Start the Remote UI, and then log in as Administrator.
"Starting the Remote UI"
2
Click [Settings/Registration].
3
Select [Network] from the [Preferences] menu.
4
Click [Ethernet Driver Settings].
5
Check the MAC address.

## Printing a Network Status Print from the Printer's Control Panel and Checking It

NOTE
###### Loading A4 paper The Network Status Print is designed to be printed on A4 paper. Be sure to load A4 paper when printing the Network Status Print.

1
Load A4 paper in the multi-purpose tray or paper drawer.
Paper Loading and Output
2
Press [ ] (: Utility).
3
Select [Network Status Print] using [ ] and [ ], then press [OK].
4
Select [Yes] using [ ], then press [OK].

| Network Status Print is printed. The MAC address (A) is indicated in [Ethernet Driver Settings] on the upper left of the Network Status Print.

0258-06W