# Changing the Remote UI Settings

Specify whether the SSL encrypted communication function should be used for the Remote UI.
1
Start the Remote UI, and then log in as Administrator.
"Starting the Remote UI"
2
Click [Settings/Registration].
3
Select [Security] from the [Management Settings] menu.
4
Click [Remote UI Settings].
5
Click [Edit...].
6
Change the Remote UI settings.

(1) | Select the [Use SSL] check box.
| If you clear the check box, the remote UI cannot use SSL encrypted communication.
(2) | Click [OK].

IMPORTANT
###### If you cannot set [Use SSL] When a key is not selected for SSL, [Use SSL] cannot be checked. Setting Keys and Certificates Selecting Keys and Certificates

7
Perform a hard reset or restart the printer.

→ | After performing a hard reset or restarting the printer, the settings are effective.

NOTE
###### To perform a hard reset You can perform a hard reset using the following procedure.
1. | Click [Settings/Registration].
2. | Select [Device Control] from the [Output/Control] menu.
3. | Select [Hard Reset], then click [Execute].

0258-0A7