# Attention (Toner Cartridge)

See "Important Safety Instructions" and "Storing Toner Cartridges" also.

IMPORTANT
###### About replacement toner cartridges For optimum print quality, using Canon genuine toner cartridges is recommended.
Model Name | Supported Canon Genuine Toner Cartridge
LBP7680Cx/LBP7660Cdn | Canon Cartridge 718 Black Canon Cartridge 718 Yellow Canon Cartridge 718 Magenta Canon Cartridge 718 Cyan
###### Be careful of counterfeit toner cartridges. Please be aware that there are counterfeit Canon toner cartridges in the marketplace. Use of counterfeit toner cartridge may result in poor print quality or machine performance. Canon is not responsible for any malfunction, accident or damage caused by the use of counterfeit toner cartridge. For more information, see http://www.canon.com/counterfeit. ###### Hold the toner cartridge properly. When handling the toner cartridge, hold it properly as shown in the figure. Do not place it vertically or upside-down. ###### Do not touch the electrical contacts (A), toner cartridge memory (B) or photoconductor drum (C). Touching the electrical contacts (A) or the toner cartridge memory (B) may cause damage. Print quality may deteriorate if you touch or scratch the photoconductor drum (C). Never touch the drum. ###### Do not touch the high-voltage contacts (D). This may result in damage to the cartridge. ###### Precautions when installing toner cartridges The position of the toner cartridges in the printer is determined by the toner color. Install the toner cartridges in the slots that have labels of the same color. ###### Other precautions Do not expose the toner cartridge to direct sunlight or strong light. Do not attempt to disassemble or modify the toner cartridge. Condensation (water droplets on the inside or outside) may form on the toner cartridge when it is brought into an environment with a sudden change in temperature or humidity. When moving a new toner cartridge to a location with change in temperature, leave the cartridge in the protective bag at the new location for two or more hours to allow it to adjust to the new temperature. Do not leave the front cover open for a long time with the toner cartridge installed. Keep toner cartridge away from products that generate magnetic waves, such as a computer or computer display.

NOTE
###### About the packing materials The packing materials may be changed in form or placement, or may be added or removed without notice.

0258-01F