# [Setup] Menu ([Interface] Options)

NOTE
###### Table description Bold values in the table indicate the default settings. After changing the setting items with "*1", cycle the power of the printer or perform a hard reset to make the settings effective. The setting items or setting values with "*2" may not be displayed depending on the availability of the optional accessories and other settings.

Setting Item | Setting Value | Setting
[Interface Selection]*1 | Specifies the settings for the interfaces used for communication with the computer or other device.
[USB] | [Use USB Connection]: [Off], [On] [Recog. USB Connect.]: [Mode 1], [Mode 2] | [Use USB Connection] Specifies whether to use the USB interface. [Recog. USB Connect.] Switches the USB connection recognition mode. Normally, set it as [Mode 1].
[Network] | [Off], [On] | Specifies whether to use the network interface.
[USB Storage Device]*2 | [MEAP Driver]: [Off], [On] | Specifies the setting for the device driver when using USB memory devices.
[Timeout] | [Timeout]: [Off], [On] [Timeout Time]: 5 to 15 to 300 seconds | Specifies the function to finish a job automatically.
[Connection Recog.]*1 | [Off], [On] | When you print using the standard network, you may not obtain proper printout results. (Unreadable characters are printed, overlay printing fails, etc.) In this case, specify [Off] for this item.
[Extended RX Buffer]*1*2 | [Off], [On] | If this item is set to [On], the memory capacity of the printer's receive buffer that receives the data is increased. You can speed up the time the computer exits when you send a large amount of data or complicated data from the computer.

0258-08X