# Network Settings for the Printer (Common to Each Protocol)

This section describes the setting items which are common to each protocol to use this printer in a network environment.

#### Selecting a Communication Method or Ethernet Type

If you want to fix the type of communication method and Ethernet type, set [Auto Detect] on the Ethernet Drive Setting to [Off]. (This printer can detect the communication method and Ethernet type automatically. Normally, you do not need to specify the setting.)
"Changing the Network Transmission Speed or Transfer Mode"

#### Specifying the Setting for Startup Waiting Time

If the printer cannot be connected to a network, see the following item and specify the setting for the startup waiting time. (Normally, you do not need to change the setting for startup waiting time.)
"Specifying the Setting for Startup Waiting Time"

#### Setting the Spooling Function (LBP7680Cx Only)

You can speed up the exiting time of the computer to which you send print jobs, see the following item and configure the spooler function.
"Setting the Spooling Function (LBP7680Cx Only)"

#### Restricting the Users Who Can Monitor and Change the Settings

If you want to restrict the users who can monitor and change the settings, see the following items and configure the SNMP protocol.
"Restricting the Users Who Can Monitor/Change the Settings Using the SNMP Protocol"

#### Setting IEEE802.1X Authentication

You can specify the settings for using IEEE802.1X authentication with the printer.
"Setting IEEE802.1X Authentication "

#### Network Setting Items

This section describes the setting items which you can change using a Web browser (Remote UI), FTP Client, or NetSpot Device Installer.
"Network Setting Items"

#### Initializing the Network Settings

You can reset the network settings for the printer to the default values.
"Initializing the Network Settings"

#### Checking the MAC Address

You can check the MAC address by printing Network Status Print.
"Checking the MAC Address"
0258-069