# Paper Jams

Before removing jammed paper, see "Attention (Paper Jams)."

When a paper jam occurs, the printer beeps, displaying the message <Paper is jammed.> in the display.

| This section describes the procedure for when [Animated Instruction] is set to [On] (default setting). If [Animated Instruction] is set to [Off], the above screen is not displayed.

Messages appear one at a time. Confirm all of them.
As the messages disappear when the cover is open, take a note of them if required.
Remove the jammed paper according to the displayed message.

Paper Jam Area | Message | Clearance Procedure
(1) Multi-purpose tray | <MP Tray area> | "Clearing Paper Jams (Multi-purpose Tray)"
(2) Drawer 1 | <Drawer 1 area> | "Clearing Paper Jams (Paper Drawer)"
(3) Drawer 2*
* | Only when the paper feeder is installed
| <Drawer 2 area> | "Clearing Paper Jams (Paper Drawer)"
(4) Back cover area | <back cover area> | "Clearing Paper Jams (Back Cover)"
(5) Output area | <Output area> | "Clearing Paper Jams (Output Area)"

0258-0C2