# Printing Coated Paper

#### Checking the Coated Papers that Can be Used

You can use the following sizes of coated papers with this printer.

Standard sizes | A4, B5, A5, Legal, Letter, and Executive
Custom paper sizes | Width 76.2 to 215.9 mm, Length 127.0 to 355.6 mm*

* | Coated paper of 210 to 220 g/m² cannot be printed using 2-sided printing.
* | When loading paper in portrait orientation (when using UFR II printer driver only): Width 127.0 to 215.9 mm, Length 127.0 to 215.9 mm

#### Loading Coated Paper

Coated paper can be loaded in the drawer or the Multi-purpose tray.
"Loading Paper in the Drawer"
"Loading Paper in the Multi-purpose Tray"

###### <Precautions when loading coated paper>

Fan the paper thoroughly and align the edges before loading it. If it is not fanned enough, multiple sheets of paper may be fed at once, causing paper jams.
When fanning or aligning the paper, try to hold the edges to avoid touching the printing surface.
Take care not to mark or stain the printing surface of the paper with fingerprints, dust, or oil. This may result in poor print quality.

#### Printing from an Application

After loading coated paper, run print.
"Configuring the Printer Driver and Printing"

| The print speed may drop when printing coated paper.

0258-0F1