# Cleaning the Outside of the Printer

Before cleaning, see "Attention (Cleaning)."

1
Turn the printer OFF, then disconnect the cables or cords from the printer.

| Shut down the printer before turning it OFF. For details on the procedure for shutting down the printer, see "Turning the Printer ON/OFF."

##### <How to disconnect the cable or cord>

USB cable* | (2) Turn the computer OFF. (3) Disconnect the cable from the printer.
LAN cable* | (4) Disconnect the cable from the printer.
Power cord | (5) Disconnect the power plug from the AC power outlet. (6) Disconnect the cord from the printer.

* | Whether the cable is connected or not varies depending on your environment.

2
Firmly wring a soft cloth dampened with water or a mild detergent diluted with water, and wipe off the dirt.
3
After wiping off the dirt, wipe the printer with a dry cloth.
4
When the printer is completely dry, connect the removed cable or cord.

##### <How to connect the cable or cord>

USB cable* | Connect to the USB connector on the printer.
LAN cable* | Connect to the LAN connector on the printer.
Power cord | (1) Plug the power cord to the power socket on the printer. (2) Plug the power plug in the AC power outlet.

* | Whether the cable is connected or not varies depending on your environment.

0258-01X