# Setting the Spooling Function (LBP7680Cx Only)

Specify the setting for the spooler function using either of the following methods.
"Performing the Configuration Using the Printer's Control Panel (the Settings to Be Performed First)"
Specify the setting for the spooler function using the control panel while checking the display on the printer.
"Changing the Settings Using Web Browser (Remote UI)"
Specify the setting for the spooler function by accessing the printer from a Web browser via the network.

IMPORTANT
###### When specifying the setting for startup waiting time first Use the printer's control panel. After configuring the TCP/IP protocol settings, you can change the settings using the Web browser (Remote UI) or FTP Client.
| Because the options which can be specified vary depending on the software, see "Network Setting Items" and use each software appropriate to the environment you are using or options that you want to specify.
###### The Spooling Function It can only be used when the SD card is installed.

NOTE
###### Changing the settings using FTP Client You can also specify the setting for startup waiting time using FTP Client. "FTP Client"

0258-0KA