# How to Specify the Settings for E-mail Print

Before performing the setup, see "Attention (How to Specify the Settings for E-mail Print)."

This section describes the procedures for registering or changing the settings using a Web browser (Remote UI).
1
Start the Remote UI, and then log in as Administrator.
"Starting the Remote UI"
2
Select [Network] under [Preferences] in the [Settings/Registration] menu.
3
Click [Edit...] on the right side of [E-Mail Print Settings].
4
Specify the settings for the e-mail print function.

##### If you want to use the POP3 protocol

[POP3 Server Name] | Specifies the name or sets the IP address of the server which receives e-mails.
[POP3 User Name] | Specifies the name of the user which receives e-mails. You can enter up to 32 alphanumeric characters.
[Set/Change Password] | Specifies the password for the name of the user which receives e-mails.
[Password] | Select the check box when setting/changing the password. You can enter up to 32 alphanumeric characters.
[Confirm] | For confirmation, enter the same [Password] again.
[POP3 RX Interval] | Set the interval for automatically connecting to the server that receives e-mail in minute units. Receive e-mail at specified intervals and print it automatically. You can set from [0] (minutes) to [90] (minutes). When it is set to [0], it does not automatically receive e-mail from the server. When it is set to [0] and when you want to connect to the server before it automatically connects to the server that receives e-mail, you can receive e-mail manually. "Receiving and Printing E-mails Manually"
[POP3 RX] | Specifies whether to enable the e-mail print function.
[POP3 Server Port Number] | Specifies the port number for the server which receives e-mails. You can specify the port number between [0] and [65535].

##### If you want to use the SMTP protocol

[SMTP RX] | When it is checked, e-mail is relayed using SMTP protocol and it is automatically received and printed.
[SMTP Server Port Number] | Specifies the port number for the server which receives e-mails. You can specify the port number between [0] and [65535].

5
Click [OK].
0258-0FJ