# Paper Creases

Perform one of the following solutions according to the cause.

#### <Cause 1>Paper is not loaded properly in the paper drawer or multi-purpose tray.

Solution | Load the paper properly. "Loading Paper in the Drawer" "Loading Paper in the Multi-purpose Tray"

#### <Cause 2> Damp paper is used.

Solution | Replace the paper with new paper in an unopened package. "Precautions for Paper"

#### <Cause 3> Appropriate paper is not being used.

Solution | Replace the paper with that which can be used with this printer. "Usable Paper"

#### <Cause 4> There is a foreign object inside the printer.

Solution | Remove the foreign object inside the printer.

#### <Cause 5> Depending on the paper type or the operating environment, the paper may be creased.

Solution 1 | Perform the following procedure in the printer driver.
1. | Display the [Paper Source] sheet.
2. | Set [Paper Type] to one of the following settings.
Currently Selected Setting | Setting to be Selected
[Plain L] | [Plain L2]
[Plain] | [Plain L]
[Plain H] | [Plain]
[Heavy 1] | [Plain H]
[Heavy 2] | [Heavy 1]
[Heavy 3] | [Heavy 2]
[Envelope H] | [Envelope]
[Coated 2] | [Coated 1]
[Coated 3] | [Coated 2]
[Coated 4] | [Coated 3]
| If you change the settings, the toner may not fix onto paper well, and the printing may come out faint.

Solution 2 | Select [Curl Correction] under [Special Print Mode] set it to [On] and print again. "[Setup] Menu ([User Maintenance] Options)"
| If you change the settings, the toner may not fix onto paper well, and the printing may come out faint.
| If you specify this setting, printing speed drops.

0258-0CH