# Changing the Network Transmission Speed or Transfer Mode

Configure the Ethernet driver for this printer using either of the following methods.
"Performing the Configuration Using the Printer's Control Panel (When You First Set it Up)"
Configure the Ethernet driver using the control panel while checking the display on the printer.
"Changing the Settings Using Web Browser (Remote UI)"
Change the settings for the Ethernet driver by accessing the printer from a Web browser via the network.

IMPORTANT
###### When configuring the interface first Use the printer's control panel. After configuring the TCP/IP protocol settings, you can change the settings for the interface using the Web browser (Remote UI).

NOTE
###### Ethernet Ethernet is a LAN standard, and this printer supports 10Base-T/100Base-TX/1000Base-T connections. When this printer is used on a network, the Ethernet driver controls the communication method and Ethernet type.

0258-06A