# [Setup] Menu ([Network] Options)

NOTE
###### Table description After changing the settings for this item, cycle the power of the printer or perform a hard reset to make the settings effective. This item is displayed only when the following condition is fulfilled. [Network] in [Interface Selection] is set to [On]. Bold values in the table indicate the default settings. The setting items or setting values with "*" may not be displayed depending on the availability of the optional accessories and other settings.

Setting Item | Setting Value | Setting
[TCP/IP Settings] | Specifies the TCP/IP setting for the print server equipped with this printer.
[IPv4 Settings] | [IPv4]: [Off], [On] | When using IPv4, set it to [On].
[IP Mode]: [Auto], [Manual] | Select the method for setting the IP address. When setting the IP address using any one of DHCP, BOOTP, or RARP, select [Auto]. When specifying the IP address to the printer directly, select [Manual].
[Protocol]*: [Use DHCP]: [Off], [On] [Use BOOTP]: [Off], [On] [Use RARP]: [Off], [On] | If you set [IP Mode] to [Auto], select which protocol you want to use. Set each of [Use DHCP], [Use BOOTP], and [Use RARP] to [On] (use) or [Off] (do not use).
[IP Address Settings]: [IP Address]: 0.0.0.0 [Subnet Mask]: 0.0.0.0 [Gateway Address]: 0.0.0.0 | Specify [IP Address], [Subnet Mask], and [Gateway Address]. For the method for entering the addresses, see "Method for entering addresses " below the table.
[DNS]: [Primary Address]: 0.0.0.0 [Secondary Address]: 0.0.0.0 | Specify [Primary Address] and [Secondary Address] for DNS. For the method for entering the addresses, see "Method for entering addresses " below the table.
* | Specify the settings for [Host Name], [Domain Name], and [DNS Dynamic Update] from the Remote UI. "Configuring the Protocol Settings"
[DHCP Option]: [Acquire Host Name]: [Off], [On] [DNS Dynamic Update]: [Off], [On] | Set DHCP options when [IP Mode] is set to [Manual] and [Use DHCP] is set to [On]. When obtaining the host name using DHCP, set [Acquire Host Name] to [On]. When updating the host name using DHCP, set [DNS Dynamic Update] to [On].
[IPv6 Settings] | [IPv6]: [Off], [On] | If you want to use IP v. 6, specify [On].
* | Specify the setting for IP v. 6 from the Remote UI. "Setting IP v. 6"
[WINS Resolution] | [Off], [On] | If you want to use WINS Resolution, specify [On].
* | Specify the following settings from the Remote UI.
| [WINS Server Address] [Scope ID] [SMB Server Name] [SMB Workgroup Name] "Configuring the Protocol Settings"
[ARP/PING] | [Off], [On] | When it is set to [On], you can change the IP address settings from the client using ARP/PING commands.
[FTP] | [FTP Print]: [Off], [On] [FTP Settings]: [Off], [On] | When it is set to [On], you can access the printer's FTP server using the FTP client and print the files. If you want to perform the settings using FTP Client, set [FTP Settings] to [On].
* | Specify the settings for [FTP Print User Name] and [Password] from the Remote UI. "Configuring the Protocol Settings"
[LPD Print] | [Off], [On] | If you want to use LPD Print, specify [On].
* | Specify the setting for [Print LPD Banner Page] from the Remote UI. "Configuring the Protocol Settings"
[RAW Print] | [Off], [On] | If you want to use RAW Print, specify [On].
* | Specify the setting for [Use Bidirectional Communication] from the Remote UI. "Configuring the Protocol Settings"
[IPP Print] | [Off], [On] | If you want to use IPP Print, specify [On].
* | Specify the settings for [IPP Authentication], [User Name], and [Password] from the Remote UI. "Configuring the Protocol Settings"
[WSD] | [WSD Print]: [Off], [On] [WSD Browsing]*: [Off], [On] [Multicast Discovery]: [Off], [On] | If you want to use WSD Print, set [WSD Print] to [On], and then specify the following settings. If you want to obtain printer information using WSD, set [WSD Browsing] to [On]. If you set [WSD Print] to [On], [WSD Browsing] is not displayed. ([WSD Browsing] is fixed at [On].) If you want to set the printer to respond to requests from multicast discovery, set [Multicast Discovery] to [On].
[HTTP] | [Off], [On] | When it is set to [On], you will be able to access the printer using HTTP. When this is set to [Off], the message appears, disallowing you to use the Remote UI or perform IPP printing.
[Proxy Settings]* | [Proxy]: [Off], [On] | If you want to use the proxy function, specify [On].
[Server Address]*: - | Enter the proxy server address to be used for the proxy function.
[Port Number]*: 0 to 80 to 99999 | Enter the port number of the proxy server to be used for the proxy function. You can specify between [0] and [99999].
[Same Domain]*: [Use Proxy], [Do Not Use Proxy] | If you want to use the proxy function also for the same domain, specify [Use Proxy].
[Proxy Authentication]*: [Off], [On] | If you want to use the proxy authentication function, specify [On].
[User Name]*: - | Enter the user name to be used for the proxy authentication. Up to 24 alphanumeric characters can be entered.
[Password]*: - | Enter the password to be used for the proxy authentication. Up to 24 alphanumeric characters can be entered.
[SNTP] | [Off], [On] | When obtaining time using the SNTP Client function, specify [On].
* | Specify the settings for [NTP Server Name] and [Polling Interval] from the Remote UI. "Configuring the Protocol Settings"
[Discovery Response] | [Off], [On] | If you want to set the printer so that it responds to searches that used the multicast discovery function, specify [On].
* | Specify the setting for [Scope Name] from the Remote UI. "Configuring the Protocol Settings"
[IPSec] | [Off], [On] | When using the IPSec function, set it to [On]. "Setting the IPSec Encryption Communication Function (LBP7680Cx Only)"
[NetWare Settings] | [NetWare]: [Off], [On] [Frame Type]*: [Auto Detect], [Ethernet II], [Ethernet 802.2], [Ethernet 802.3], [Ethernet SNAP] [Print Service]*: [Bindery PServer], [RPrinter], [NDS PServer], [NPrinter] | Configures the NetWare network settings. "Configuring the Protocol Settings"
[AppleTalk] | [Off], [On] | Specifies whether the printer should use AppleTalk. "Configuring the Protocol Settings"
[SMB]* | [SMB Server]: [Off], [On] [SMB Print]: [Off], [On] | Specifies whether the printer should use SMB. "Network Settings for the Printer (SMB) (LBP7680Cx Only)"
[SNMP Settings] | Specify the settings related to SNMP protocol. "Restricting the Users Who Can Monitor/Change the Settings Using the SNMP Protocol"
[SNMP v. 1 Settings] | Specify the settings related to SNMP v. 1 protocol.
[SNMP v. 1] | [Off], [On] | Specify whether to use the SNMP v. 1 protocol.
[Dctd. Community Set.] | [Dctd. Community 1]: [Off], [Read/Write], [Read Only] [Dctd. Community 2]: [Off], [Read/Write], [Read Only] | [Dctd. Community 1] Specifies access privileges for the Management Information Base (MIB) of the community (canon_admin) that SNMP manages. [Dctd. Community 2] Specifies access privileges for the Management Information Base (MIB) of the community (canon_user) that SNMP manages.
[SNMP v. 3 Settings] | [SNMP v. 3]: [Off], [On] [User Settings 1] to [User Settings 5]*: [Auth. Password] [Encryption Password] | Specify the settings related to SNMP v. 3 protocol.
[Rjct Packet in Sleep] | [Off], [On] | Specifies whether to discard the SNMP packets received while in sleep mode.
| If you set this item to [On], you may be unable to access the printer from Canon software (iW Series) or applications using the SNMP protocol.
[Spooler]* | [Off], [On] | When using the spooling function, set it to [On]. "Setting the Spooling Function (LBP7680Cx Only)"
[Network Delay Time]* | 0 to 300 seconds | Specifies the time interval from when the printer is turned ON to when the protocol starts. "Specifying the Setting for Startup Waiting Time"
[Remote UI Settings] | [Remote UI]: [Off], [On] [SSL]*: [Off], [On]* | Specifies whether the printer should use the Remote UI. Also, whether to use SSL for communication by the Remote UI is specified. "Setting Keys and Certificates"
[Ethernet Driver]* | [Auto Detect]: [Off], [On] [Communication Mode]*: [Half Duplex], [Full Duplex] [Ethernet Type]*: [10 Base-T], [100 Base-TX], [1000 Base-T] | Configures the Ethernet driver. "Changing the Network Transmission Speed or Transfer Mode"
[IEEE802.1X] | [Off], [On] | When using the IEEE802.1X function, set it to [On]. "Setting IEEE802.1X Authentication "
[Address Filter] | [Off], [On] | When using the address filter function, set it to [On]. "Restricting the Users Who Can Print or Perform the Printer Settings" "Restricting the Users Who Can Access"
[MAC Address]* | (Display only) | Displays the MAC address of the printer.
[E-Mail Print Set.] | [POP3 RX Interval]: 0 to 90 (minutes) [POP3 RX]: [Off], [On] [SMTP RX]: [Off], [On] | Set e-mail print. "Receiving E-mail Data on the Mail Server and Printing (E-mail Print)"
[Init. Network Set.] | - | By the initialization in this item, you can reset the network settings to the default settings. "Initializing the Network Settings"

##### Method for entering addresses

1. | Move the cursor to each field (an area separated by periods to enter three-digit numbers) in which you want to enter the address, by pressing [ ] or [ ]. (The number in the field blinks, allowing you to enter a value.)
2. | Enter the numbers. ([ ] increases the value and [ ] decreases the value.)
3. | After entering values in all the fields, press [OK] to confirm the settings.

0258-08S